{"payload":{"meta":{"Graph":{"@Type":"81297157","@Value":{"Guid":"(Guid)b88b9b8d-9ba7-401a-b785-01ebd17fa645","ParentGuid":"(Guid)74ccca2f-50e3-4d5a-9d7a-9fd420284f83","Name":"(string)atHumidityCtl","Properties":{"@Type":"2c41fa04:IDictionary","@Value":[{"@Key":"(Guid)829a18f2-c514-4f6e-9634-1df173429203","@Value":{"@Type":"829a18f2","@Value":{"ParentObjects":{"@Type":"fa2ee218:IDictionary","@Value":[{"@Key":"(Guid)d9b2b2cc-ea99-4c3b-aa42-1e5c49e65b84","@Value":"(Guid)510e2535-b7c5-42ba-af61-e3dfb58c63d4"}]}}}}]},"TypeGuid":"(Guid)6f9dac99-8de1-4efc-8465-68ac443b7d08","EmbeddedTypeGuids":{"@Type":"[Guid]","@Value":["(Guid)a9ed5b7e-75c5-4651-af16-d2c27e98cb94","(Guid)3b83b776-fb25-43b8-99f2-3c507c9143fc"]}}},"TypeInfos":{"2c41fa04":"{2c41fa04-1834-41c1-816e-303c7aa2c05b}","81297157":"{81297157-7ec9-45ce-845e-84cab2b88ade}","829a18f2":"{829a18f2-c514-4f6e-9634-1df173429203}","fa2ee218":"{fa2ee218-a39b-4b6d-b249-49dbddbd168a}","Guid":"System.Guid","string":"System.String"}},"object":{"Graph":{"@Type":"6f9dac99","@Value":{"SpecialFunc":{"@Type":"0db3d7bb:Enum","@Value":"None"},"Implementation":{"@Type":"3b83b776","@Value":{"TextDocument":{"@Type":"f3878285","@Value":{"TextBlobForSerialisation":"(string)//   --- Turns the Humidity Controls off when out of range of set value ---\nbelow := in_hu < lo;\n\n//   --- Indicator for letting the user see when somthing is being driven via humidity ctl vs stage ctl ---\nhu := in_hu > lo;\n\nratioScaling(\n\tin_raw := in_hu,\n\tin_clamp := TRUE,\n\tin_rawMin := lo, \n\tin_rawMax := hi, \n\tout_eu => Ratio);\n\t\n\tFOR i := 0 TO DINT_TO_INT (UPPER_BOUND(variableDev,1)) DO\n\t\tvariableDev[i](in_ratio := ratio, underRange := below);\n\tEND_FOR\n\t\n\t//   --- Designated for Heat Mixing or Heat Circ Fans---\n\tvariableDev[0].in_name := 'Heat Mixing Valve';\t\t\t\t\t\t//Variable Dev [0] - [1] and Designated for Heating so the outputs are flipped\n\tvariableDev[0].outputScaling(in_rawMax := 100, in_rawMin := 0);\t\t//Variable Dev [0] - [1] and Designated for Heating so the outputs are flipped\n\tvariableDev[1].in_name := 'Heat Circ Fans';\t\t\t\t\t\t\t//Variable Dev [0] - [1] and Designated for Heating so the outputs are flipped\n\tvariableDev[1].outputScaling(in_rawMax := 100, in_rawMin := 0);\t\t//Variable Dev [0] - [1] and Designated for Heating so the outputs are flipped\n\t\n\t//   --- Fixed Device Control ---\n\tfixedDev[0](in_ratio := ratio,underRange := below);\n\tfixedDev[1](in_ratio := ratio,underRange := below);\n\tfixedDev[2](in_ratio := ratio,underRange := below);\n\n\t\n\t\n\t","LineInfoPersistence":"(string)b88b9b8d-9ba7-401a-b785-01ebd17fa645_Impl_LineIds"}}}},"Interface":{"@Type":"a9ed5b7e","@Value":{"TextDocument":{"@Type":"f3878285","@Value":{"TextBlobForSerialisation":"(string){attribute 'no_assign'}\nFUNCTION_BLOCK atHumidityCtl\nVAR_INPUT\n\tvariableDev: ARRAY[0..10] OF atHumidityVari;\n\tfixedDev: ARRAY[0..2] OF atHumidityFixed;\n\tin_hu: REAL;\nEND_VAR\nVAR_INPUT PERSISTENT\n\thi: REAL;\t\t\t//Hi Humidity setpoint\n\tlo: REAL;\t\t\t//Lo Humidity setpoint\nEND_VAR\nVAR\n\ti: INT;\n\tratioScaling: atScaling;\n\tratio: REAL;\n\tbelow: BOOL;\nEND_VAR\nVAR_OUTPUT\n\thu: BOOL;\nEND_VAR\n","LineInfoPersistence":"(string)b88b9b8d-9ba7-401a-b785-01ebd17fa645_Decl_LineIds"}}}},"UniqueIdGenerator":"(string)328","POULevel":{"@Type":"8e575c5b:Enum","@Value":"Standard"},"ChildObjectGuids":{"@Type":"ArrayList:IList","@Value":[]},"AddAttributeSubsequent":"(bool)False"}},"TypeInfos":{"0db3d7bb":"{0db3d7bb-cde0-4416-9a7b-ce49a0124323}","3b83b776":"{3b83b776-fb25-43b8-99f2-3c507c9143fc}","6f9dac99":"{6f9dac99-8de1-4efc-8465-68ac443b7d08}","8e575c5b":"{8e575c5b-1d37-49c6-941b-5c0ec7874787}","a9ed5b7e":"{a9ed5b7e-75c5-4651-af16-d2c27e98cb94}","ArrayList":"System.Collections.ArrayList","bool":"System.Boolean","f3878285":"{f3878285-8e4f-490b-bb1b-9acbb7eb04db}","string":"System.String"}}},"FormatVersion":"1.0"}