{"payload":{"meta":{"Graph":{"@Type":"81297157","@Value":{"Guid":"(Guid)aee2e3b2-613a-43a6-9d55-49665a11a515","ParentGuid":"(Guid)74ccca2f-50e3-4d5a-9d7a-9fd420284f83","Name":"(string)atStageCtrl","Properties":{"@Type":"2c41fa04:IDictionary","@Value":[{"@Key":"(Guid)829a18f2-c514-4f6e-9634-1df173429203","@Value":{"@Type":"829a18f2","@Value":{"ParentObjects":{"@Type":"fa2ee218:IDictionary","@Value":[{"@Key":"(Guid)d9b2b2cc-ea99-4c3b-aa42-1e5c49e65b84","@Value":"(Guid)c598b144-c84a-47fb-92dd-880c1019a03a"}]}}}}]},"TypeGuid":"(Guid)6f9dac99-8de1-4efc-8465-68ac443b7d08","EmbeddedTypeGuids":{"@Type":"[Guid]","@Value":["(Guid)a9ed5b7e-75c5-4651-af16-d2c27e98cb94","(Guid)3b83b776-fb25-43b8-99f2-3c507c9143fc"]}}},"TypeInfos":{"2c41fa04":"{2c41fa04-1834-41c1-816e-303c7aa2c05b}","81297157":"{81297157-7ec9-45ce-845e-84cab2b88ade}","829a18f2":"{829a18f2-c514-4f6e-9634-1df173429203}","fa2ee218":"{fa2ee218-a39b-4b6d-b249-49dbddbd168a}","Guid":"System.Guid","string":"System.String"}},"object":{"Graph":{"@Type":"6f9dac99","@Value":{"SpecialFunc":{"@Type":"0db3d7bb:Enum","@Value":"None"},"Implementation":{"@Type":"3b83b776","@Value":{"TextDocument":{"@Type":"f3878285","@Value":{"TextBlobForSerialisation":"(string)//Calculates the active stage given stage setpoints, a setpoint temperature and the current temperature\n//2024-01-29 CWD Initial create \n\n//Calculate the setpoints for each stage\nFOR i := LOWER_BOUND(stages,1) TO UPPER_BOUND(stages,1) DO\n\t\tstages[i].SP := setpoint + stages[i].Offset;\n\t\tstages[i].hiSP := stages[i].SP + stages[i].Span / 2;\n\t\tstages[i].lowSP := stages[i].SP - stages[i].Span / 2;\nEND_FOR\n\n//Check the stage above the currently active stage to see if it should be active\n//If temperature is more then 1/2 way through the next stage then set the index to the next stage\nIF activeIdx < UPPER_BOUND(stages,1) THEN //only change idx if there is another one\n\tnextStage := stages[activeIdx+1];\n\tIF in >= nextStage.SP THEN\n\t\tactiveIdx := activeIdx + 1;\n\tEND_IF\nEND_IF\n\n//If temperature is less the 1/2 way through the previous stage then set index to the previous stage\nIF activeIdx > LOWER_BOUND(stages,1) THEN //only change idx if there is another one\n\tprevStage := stages[activeIdx-1];\n\tIF in <= prevStage.SP THEN\n\t\tactiveIdx := activeIdx - 1;\n\tEND_IF\nEND_IF\n\n//Set active stage based on index\nactiveStage := stages[activeIdx];\n","LineInfoPersistence":"(string)aee2e3b2-613a-43a6-9d55-49665a11a515_Impl_LineIds"}}}},"Interface":{"@Type":"a9ed5b7e","@Value":{"TextDocument":{"@Type":"f3878285","@Value":{"TextBlobForSerialisation":"(string)FUNCTION_BLOCK atStageCtrl\nVAR_INPUT\n\t// Input temperature\n\tin: REAL;\n\t// Setpoint temperature\n\tsetpoint: REAL;\nEND_VAR\nVAR_IN_OUT\n\t// List of stage settings\n\tstages: ARRAY[*] OF atStageSP;\nEND_VAR\nVAR_OUTPUT\n\t// currently active stage\n\tactiveStage: atStageSP;\n\t// active stage index\n\tactiveIdx: INT := 0;\nEND_VAR\nVAR\n\t// loop index\n\ti: DINT;\n\n\tnextStage: atStageSP;\n\tprevStage: atStageSP;\nEND_VAR\n","LineInfoPersistence":"(string)aee2e3b2-613a-43a6-9d55-49665a11a515_Decl_LineIds"}}}},"UniqueIdGenerator":"(string)590","POULevel":{"@Type":"8e575c5b:Enum","@Value":"Standard"},"ChildObjectGuids":{"@Type":"ArrayList:IList","@Value":[]},"AddAttributeSubsequent":"(bool)False"}},"TypeInfos":{"0db3d7bb":"{0db3d7bb-cde0-4416-9a7b-ce49a0124323}","3b83b776":"{3b83b776-fb25-43b8-99f2-3c507c9143fc}","6f9dac99":"{6f9dac99-8de1-4efc-8465-68ac443b7d08}","8e575c5b":"{8e575c5b-1d37-49c6-941b-5c0ec7874787}","a9ed5b7e":"{a9ed5b7e-75c5-4651-af16-d2c27e98cb94}","ArrayList":"System.Collections.ArrayList","bool":"System.Boolean","f3878285":"{f3878285-8e4f-490b-bb1b-9acbb7eb04db}","string":"System.String"}}},"FormatVersion":"1.0"}