{"payload":{"meta":{"Graph":{"@Type":"81297157","@Value":{"Guid":"(Guid)e86b29ba-eef7-47e4-87c8-e2721d5fe17b","ParentGuid":"(Guid)74ccca2f-50e3-4d5a-9d7a-9fd420284f83","Name":"(string)atMbReqReadHolding","Properties":{"@Type":"2c41fa04:IDictionary","@Value":[{"@Key":"(Guid)829a18f2-c514-4f6e-9634-1df173429203","@Value":{"@Type":"829a18f2","@Value":{"ParentObjects":{"@Type":"fa2ee218:IDictionary","@Value":[{"@Key":"(Guid)d9b2b2cc-ea99-4c3b-aa42-1e5c49e65b84","@Value":"(Guid)1cccc206-fde4-465c-8b3d-b850f842be99"}]}}}}]},"TypeGuid":"(Guid)6f9dac99-8de1-4efc-8465-68ac443b7d08","EmbeddedTypeGuids":{"@Type":"[Guid]","@Value":["(Guid)a9ed5b7e-75c5-4651-af16-d2c27e98cb94","(Guid)3b83b776-fb25-43b8-99f2-3c507c9143fc"]}}},"TypeInfos":{"2c41fa04":"{2c41fa04-1834-41c1-816e-303c7aa2c05b}","81297157":"{81297157-7ec9-45ce-845e-84cab2b88ade}","829a18f2":"{829a18f2-c514-4f6e-9634-1df173429203}","fa2ee218":"{fa2ee218-a39b-4b6d-b249-49dbddbd168a}","Guid":"System.Guid","string":"System.String"}},"object":{"Graph":{"@Type":"6f9dac99","@Value":{"SpecialFunc":{"@Type":"0db3d7bb:Enum","@Value":"None"},"Implementation":{"@Type":"3b83b776","@Value":{"TextDocument":{"@Type":"f3878285","@Value":{"TextBlobForSerialisation":"(string)//Modbus request input registers\n//2024-06-27 CWD Initial Create\n//2024-10-21 CWD Set udiTimeout to 0 as this was causing problems with detecting an actual no reply timeout from the slave \n//2024-11-15 ATM Moved from Work to main for easier debugging\n//2024-11-23 ATM Cleaned up code, added start array position\n\n\n//Verify data size is large enough, if not then only get as many registers that will fit.\ndataSize := UPPER_BOUND(data,1) - LOWER_BOUND(data,1) + 1;  \n\n//Do all class work\nSUPER^();\n\n//Do request processing\nrequest(\n\trClient := mbsClient, \n\txExecute := execute, \n\tudiTimeOut := 0,\n\tuiUnitId := in_unitId,\n\tudiReplyTimeout := replyTimeout,\n\tuiStartItem := in_startAddr, \n\tuiQuantity := quantUsed, \n\tpData := ADR(data[in_dataOffset])\n);\n\nDone(request.xDone);\nError(request.xError);\n\t","LineInfoPersistence":"(string)e86b29ba-eef7-47e4-87c8-e2721d5fe17b_Impl_LineIds"}}}},"Interface":{"@Type":"a9ed5b7e","@Value":{"TextDocument":{"@Type":"f3878285","@Value":{"TextBlobForSerialisation":"(string){attribute 'no_assign'}\nFUNCTION_BLOCK atMbReqReadHolding EXTENDS atMbReqBase\nVAR_IN_OUT\n\t// ARRAY[] OF UINT to hold received data\n\tdata: ARRAY[*] OF UINT;\nEND_VAR\nVAR_OUTPUT\nEND_VAR\nVAR\n    {attribute 'symbol' := 'none'}\n\trequest: ModbusFB.ClientRequestReadHoldingRegisters;\nEND_VAR\n","LineInfoPersistence":"(string)e86b29ba-eef7-47e4-87c8-e2721d5fe17b_Decl_LineIds"}}}},"UniqueIdGenerator":"(string)141","POULevel":{"@Type":"8e575c5b:Enum","@Value":"Standard"},"ChildObjectGuids":{"@Type":"ArrayList:IList","@Value":[]},"AddAttributeSubsequent":"(bool)False"}},"TypeInfos":{"0db3d7bb":"{0db3d7bb-cde0-4416-9a7b-ce49a0124323}","3b83b776":"{3b83b776-fb25-43b8-99f2-3c507c9143fc}","6f9dac99":"{6f9dac99-8de1-4efc-8465-68ac443b7d08}","8e575c5b":"{8e575c5b-1d37-49c6-941b-5c0ec7874787}","a9ed5b7e":"{a9ed5b7e-75c5-4651-af16-d2c27e98cb94}","ArrayList":"System.Collections.ArrayList","bool":"System.Boolean","f3878285":"{f3878285-8e4f-490b-bb1b-9acbb7eb04db}","string":"System.String"}}},"FormatVersion":"1.0"}