{"payload":{"meta":{"Graph":{"@Type":"81297157","@Value":{"Guid":"(Guid)1229a8f4-4d09-419c-8685-01c57e6f1900","ParentGuid":"(Guid)74ccca2f-50e3-4d5a-9d7a-9fd420284f83","Name":"(string)atTeAI","Properties":{"@Type":"2c41fa04:IDictionary","@Value":[{"@Key":"(Guid)829a18f2-c514-4f6e-9634-1df173429203","@Value":{"@Type":"829a18f2","@Value":{"ParentObjects":{"@Type":"fa2ee218:IDictionary","@Value":[{"@Key":"(Guid)d9b2b2cc-ea99-4c3b-aa42-1e5c49e65b84","@Value":"(Guid)d07cae46-81dc-4312-a96a-30735d20d93d"}]}}}}]},"TypeGuid":"(Guid)6f9dac99-8de1-4efc-8465-68ac443b7d08","EmbeddedTypeGuids":{"@Type":"[Guid]","@Value":["(Guid)a9ed5b7e-75c5-4651-af16-d2c27e98cb94","(Guid)3b83b776-fb25-43b8-99f2-3c507c9143fc"]}}},"TypeInfos":{"2c41fa04":"{2c41fa04-1834-41c1-816e-303c7aa2c05b}","81297157":"{81297157-7ec9-45ce-845e-84cab2b88ade}","829a18f2":"{829a18f2-c514-4f6e-9634-1df173429203}","fa2ee218":"{fa2ee218-a39b-4b6d-b249-49dbddbd168a}","Guid":"System.Guid","string":"System.String"}},"object":{"Graph":{"@Type":"6f9dac99","@Value":{"SpecialFunc":{"@Type":"0db3d7bb:Enum","@Value":"None"},"Implementation":{"@Type":"3b83b776","@Value":{"TextDocument":{"@Type":"f3878285","@Value":{"TextBlobForSerialisation":"(string)//2025-04-03 ATM Changed to extending ai\n\nIF NOT in_ready THEN\n\tout_ready := FALSE;\n\tRETURN;\nEND_IF\n\n//This could be delayed until filter has had time to work\nout_ready := TRUE;\nIF in_simEn THEN\n\tout_eu := in_simIn;\nELSE\n\tgetFaults();\n\tdoScalingRaw();\n\tdoScalingEU();\n\tte1_res := atVoltageDivider(in_voltsOut := scalingEU.out_eu, in_supplyVolts := in_supVlt, in_resistor := in_resVal);\n\tout_scaled := atTherm2(Ohms := te1_res, ThermType := in_thermType);\n\tdoFiltering();\n\tout_eu := filtered;\n\tIF faults.chan.out_unlatched THEN\n\t\tout_eu := -999;\n\tEND_IF\nEND_IF\n\ndoLimits();\n","LineInfoPersistence":"(string)1229a8f4-4d09-419c-8685-01c57e6f1900_Impl_LineIds"}}}},"Interface":{"@Type":"a9ed5b7e","@Value":{"TextDocument":{"@Type":"f3878285","@Value":{"TextBlobForSerialisation":"(string){attribute 'no_assign'}\nFUNCTION_BLOCK atTeAI EXTENDS atAI\nVAR_INPUT PERSISTENT\n\tin_thermType: INT;\t\t//Therm Type (i.e 1 = 3K)\n\tin_resVal: INT;\t\t\t//Resistor Value (i.e. 3267)\n\tin_supVlt: REAL;\t\t\t//In Supply Voltage \nEND_VAR\nVAR\n\tte1_res: REAL;\nEND_VAR","LineInfoPersistence":"(string)1229a8f4-4d09-419c-8685-01c57e6f1900_Decl_LineIds"}}}},"UniqueIdGenerator":"(string)274","POULevel":{"@Type":"8e575c5b:Enum","@Value":"Standard"},"ChildObjectGuids":{"@Type":"ArrayList:IList","@Value":[]},"AddAttributeSubsequent":"(bool)False"}},"TypeInfos":{"0db3d7bb":"{0db3d7bb-cde0-4416-9a7b-ce49a0124323}","3b83b776":"{3b83b776-fb25-43b8-99f2-3c507c9143fc}","6f9dac99":"{6f9dac99-8de1-4efc-8465-68ac443b7d08}","8e575c5b":"{8e575c5b-1d37-49c6-941b-5c0ec7874787}","a9ed5b7e":"{a9ed5b7e-75c5-4651-af16-d2c27e98cb94}","ArrayList":"System.Collections.ArrayList","bool":"System.Boolean","f3878285":"{f3878285-8e4f-490b-bb1b-9acbb7eb04db}","string":"System.String"}}},"FormatVersion":"1.0"}