{"payload":{"meta":{"Graph":{"@Type":"81297157","@Value":{"Guid":"(Guid)64ddbe44-1bd1-43c8-a067-8737ee14af4f","ParentGuid":"(Guid)74ccca2f-50e3-4d5a-9d7a-9fd420284f83","Name":"(string)atMbClientRTU","Properties":{"@Type":"2c41fa04:IDictionary","@Value":[{"@Key":"(Guid)829a18f2-c514-4f6e-9634-1df173429203","@Value":{"@Type":"829a18f2","@Value":{"ParentObjects":{"@Type":"fa2ee218:IDictionary","@Value":[{"@Key":"(Guid)d9b2b2cc-ea99-4c3b-aa42-1e5c49e65b84","@Value":"(Guid)1cccc206-fde4-465c-8b3d-b850f842be99"}]}}}}]},"TypeGuid":"(Guid)6f9dac99-8de1-4efc-8465-68ac443b7d08","EmbeddedTypeGuids":{"@Type":"[Guid]","@Value":["(Guid)a9ed5b7e-75c5-4651-af16-d2c27e98cb94","(Guid)3b83b776-fb25-43b8-99f2-3c507c9143fc"]}}},"TypeInfos":{"2c41fa04":"{2c41fa04-1834-41c1-816e-303c7aa2c05b}","81297157":"{81297157-7ec9-45ce-845e-84cab2b88ade}","829a18f2":"{829a18f2-c514-4f6e-9634-1df173429203}","fa2ee218":"{fa2ee218-a39b-4b6d-b249-49dbddbd168a}","Guid":"System.Guid","string":"System.String"}},"object":{"Graph":{"@Type":"6f9dac99","@Value":{"SpecialFunc":{"@Type":"0db3d7bb:Enum","@Value":"None"},"Implementation":{"@Type":"3b83b776","@Value":{"TextDocument":{"@Type":"f3878285","@Value":{"TextBlobForSerialisation":"(string)//Modbus connection\n//Connects to a modbus slave\n//2024-06-27 CWD Initial create\n//2024-11-13 CWD Fix problem with not connecting properly on power up\n//2024-11-15 ATM Move from structure to defaults.\n//2024-11-23 ATM Cleaned up code\n\nIF NOT initDone THEN\n\tinitDone := TRUE;\n\n\t//Initially set xConnect true, then set to false below to reset port. Otherwise on reboot the port will appear to be working, but will have comm timeouts\n\t_client.xConnect := TRUE;\n\n\t//Other configuration parameters \n\t_client.iPort := in_port;\n\t_client.dwBaudrate := in_baudRate; \n\t_client.byDataBits := in_dataBits; \n\t_client.eParity := in_parity;\n\t_client.eStopBits := in_stopBits; \n\t_client.eDTRcontrol := 0; \n\t_client.eRTScontrol := 0; \n\t_client.eRTUASCII := 0; \n\t_client.udiLogOptions := ModbusFB.LoggingOptions.None;\n\t_client();\n\t\n\t//Set xConnect back to false to complete the init process\n\t_client.xConnect:=FALSE; \n\t\nEND_IF\n\nclient REF= _client;\n\nSUPER^();","LineInfoPersistence":"(string)64ddbe44-1bd1-43c8-a067-8737ee14af4f_Impl_LineIds"}}}},"Interface":{"@Type":"a9ed5b7e","@Value":{"TextDocument":{"@Type":"f3878285","@Value":{"TextBlobForSerialisation":"(string){attribute 'no_assign'}\nFUNCTION_BLOCK atMbClientRTU EXTENDS atMbClient\nVAR_INPUT\n\tin_port: BYTE := 0; //0=None, 1,2,3,4\n\tin_baudRate: UINT := 9600; //4800, 9600, 19200, 38400, 57600, 115200\n\tin_parity: BYTE := 0; //0=None, 1=Odd, 2=Even\n\tin_dataBits: BYTE := 8; //8=8\n\tin_stopBits: BYTE := 1; //1=OneStopBit, 2=One5StopBits, 3=TwoStopBits\nEND_VAR\nVAR\n    {attribute 'symbol' := 'none'}\n\t_client: ModbusFB.ClientSerial;\nEND_VAR","LineInfoPersistence":"(string)64ddbe44-1bd1-43c8-a067-8737ee14af4f_Decl_LineIds"}}}},"UniqueIdGenerator":"(string)545","POULevel":{"@Type":"8e575c5b:Enum","@Value":"Standard"},"ChildObjectGuids":{"@Type":"ArrayList:IList","@Value":[]},"AddAttributeSubsequent":"(bool)False"}},"TypeInfos":{"0db3d7bb":"{0db3d7bb-cde0-4416-9a7b-ce49a0124323}","3b83b776":"{3b83b776-fb25-43b8-99f2-3c507c9143fc}","6f9dac99":"{6f9dac99-8de1-4efc-8465-68ac443b7d08}","8e575c5b":"{8e575c5b-1d37-49c6-941b-5c0ec7874787}","a9ed5b7e":"{a9ed5b7e-75c5-4651-af16-d2c27e98cb94}","ArrayList":"System.Collections.ArrayList","bool":"System.Boolean","f3878285":"{f3878285-8e4f-490b-bb1b-9acbb7eb04db}","string":"System.String"}}},"FormatVersion":"1.0"}