{"payload":{"meta":{"Graph":{"@Type":"81297157","@Value":{"Guid":"(Guid)58306787-1dd9-4c62-b8ad-d16f6b51669e","ParentGuid":"(Guid)74ccca2f-50e3-4d5a-9d7a-9fd420284f83","Name":"(string)atVarFanOld","Properties":{"@Type":"2c41fa04:IDictionary","@Value":[{"@Key":"(Guid)829a18f2-c514-4f6e-9634-1df173429203","@Value":{"@Type":"829a18f2","@Value":{"ParentObjects":{"@Type":"fa2ee218:IDictionary","@Value":[{"@Key":"(Guid)d9b2b2cc-ea99-4c3b-aa42-1e5c49e65b84","@Value":"(Guid)c598b144-c84a-47fb-92dd-880c1019a03a"}]}}}}]},"TypeGuid":"(Guid)6f9dac99-8de1-4efc-8465-68ac443b7d08","EmbeddedTypeGuids":{"@Type":"[Guid]","@Value":["(Guid)a9ed5b7e-75c5-4651-af16-d2c27e98cb94","(Guid)3b83b776-fb25-43b8-99f2-3c507c9143fc"]}}},"TypeInfos":{"2c41fa04":"{2c41fa04-1834-41c1-816e-303c7aa2c05b}","81297157":"{81297157-7ec9-45ce-845e-84cab2b88ade}","829a18f2":"{829a18f2-c514-4f6e-9634-1df173429203}","fa2ee218":"{fa2ee218-a39b-4b6d-b249-49dbddbd168a}","Guid":"System.Guid","string":"System.String"}},"object":{"Graph":{"@Type":"6f9dac99","@Value":{"SpecialFunc":{"@Type":"0db3d7bb:Enum","@Value":"None"},"Implementation":{"@Type":"3b83b776","@Value":{"TextDocument":{"@Type":"f3878285","@Value":{"TextBlobForSerialisation":"(string)//Calculates the Run demand and speed output for a variable speed fan\n//2024-01-24 CWD Initial create\n\n//Run demand is based on one of the control or fixed speed being enabled\n//Speed is high selected from all controlers\n//There could be many control speeds. In this case we use 2. Control speeds are calculated speeds based on temperature, humidity, or other schemes.\nrunEn := FALSE;\nspeedDem := 0;\n\n//Loop for each control speed\nFOR I:= 0 TO 1 DO\n\tIF stage.VarFanSP[fanIdx].CtrlEn[i] THEN\n\t\trunEn := TRUE;\n\t\tspeedDem := atHighSelect(in1 := speedDem, in2 := ctrlSpeed[i]);\n\tEND_IF\nEND_FOR\n\n//Fixed speed\nIF stage.VarFanSP[fanIdx].FixedEn THEN\n\trunEn := TRUE;\n\tspeedDem := atHighSelect(in1 := speedDem, in2 := stage.VarFanSP[fanIdx].FixedSP);\nEND_IF","LineInfoPersistence":"(string)58306787-1dd9-4c62-b8ad-d16f6b51669e_Impl_LineIds"}}}},"Interface":{"@Type":"a9ed5b7e","@Value":{"TextDocument":{"@Type":"f3878285","@Value":{"TextBlobForSerialisation":"(string)FUNCTION_BLOCK atVarFanOld\nVAR_INPUT\n\tstage: atStageSP;\n\tfanIdx: INT;\n\tctrlSpeed: ARRAY[0..1] OF REAL;\nEND_VAR\nVAR_OUTPUT\n\trunEn: BOOL;\nEND_VAR\nVAR\n\ti: INT;\nEND_VAR\nVAR_OUTPUT\n\tspeedDem: REAL;\nEND_VAR\n","LineInfoPersistence":"(string)58306787-1dd9-4c62-b8ad-d16f6b51669e_Decl_LineIds"}}}},"UniqueIdGenerator":"(string)269","POULevel":{"@Type":"8e575c5b:Enum","@Value":"Standard"},"ChildObjectGuids":{"@Type":"ArrayList:IList","@Value":[]},"AddAttributeSubsequent":"(bool)False"}},"TypeInfos":{"0db3d7bb":"{0db3d7bb-cde0-4416-9a7b-ce49a0124323}","3b83b776":"{3b83b776-fb25-43b8-99f2-3c507c9143fc}","6f9dac99":"{6f9dac99-8de1-4efc-8465-68ac443b7d08}","8e575c5b":"{8e575c5b-1d37-49c6-941b-5c0ec7874787}","a9ed5b7e":"{a9ed5b7e-75c5-4651-af16-d2c27e98cb94}","ArrayList":"System.Collections.ArrayList","bool":"System.Boolean","f3878285":"{f3878285-8e4f-490b-bb1b-9acbb7eb04db}","string":"System.String"}}},"FormatVersion":"1.0"}