{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Alarms"],"not_rendered":{"comments":1},"read":"whole","date_system":"1900"}

{"sheet":"Alarms","index":0,"n_rows":32,"n_cols":14,"rows_kept":32}
["id","description","siteId","deviceId","calculation","updateInterval","message","messageRtn","importanceLevel","latching","delayOn","delayOff","enabled","alarmGroupIds"]
[]
["water_g_bs1_cd1_fault_out","IO Base 1 Card 1 Fault","rosebud_feeders","mill","|{register:mill:water_g_bs1_cd1_fault_out}|",1,"IO Base 1 Card 1 Communication Fault","RTN - IO Base 1 Card 1 Communication Restored",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_bs1_cd2_fault_out","IO Base 1 Card 2 Fault","rosebud_feeders","mill","|{register:mill:water_g_bs1_cd2_fault_out}|",1,"IO Base 1 Card 2 Communication Fault","RTN - IO Base 1 Card 2 Communication Restored",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_cysNoPress_faults_chan_out","Cistern Pressure IO Channel Fault","rosebud_feeders","mill","|{register:mill:water_g_cysNoPress_faults_chan_out}|",1,"Cistern Pressure IO Channel Fault","RTN - Cistern Pressure IO Channel OK",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_cysNoPress_alm_out","Cistern No Pressure Alarm","rosebud_feeders","mill","|{register:mill:water_g_cysNoPress_alm_out}|",1,"South West Water Shack Pressure Low","RTN - South West Water Shack Pressure OK",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_well4Vol_fault_out","Well 4 Volume Meter Fault","rosebud_feeders","mill","|{register:mill:water_g_well4Vol_fault_out}|",1,"Well 4 Volume Meter Communication Fault","RTN - Well 4 Volume Meter Communication Restored",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_well4IO_cd1_fault_out","Well 4 IO Card 1 Fault","rosebud_feeders","mill","|{register:mill:water_g_well4IO_cd1_fault_out}|",1,"Well 4 IO Card 1 Communication Fault","RTN - Well 4 IO Card 1 Communication Restored",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_cysLevel_faults_over_out","Cistern Level Over-Range Fault","rosebud_feeders","mill","|{register:mill:water_g_cysLevel_faults_over_out}|",1,"Cistern Level Signal Over Range","RTN - Cistern Level Signal Normal",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_cysLevel_faults_under_out","Cistern Level Under-Range Fault","rosebud_feeders","mill","|{register:mill:water_g_cysLevel_faults_under_out}|",1,"Cistern Level Signal Under Range","RTN - Cistern Level Signal Normal",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_cysLevel_faults_chan_out","Cistern Level IO Channel Fault","rosebud_feeders","mill","|{register:mill:water_g_cysLevel_faults_chan_out}|",1,"Cistern Level IO Channel Fault","RTN - Cistern Level IO Channel OK",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_cysPress_faults_over_out","Cistern Pressure Over-Range Fault","rosebud_feeders","mill","|{register:mill:water_g_cysPress_faults_over_out}|",1,"Cistern Pressure Signal Over Range","RTN - Cistern Pressure Signal Normal",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_cysPress_faults_under_out","Cistern Pressure Under-Range Fault","rosebud_feeders","mill","|{register:mill:water_g_cysPress_faults_under_out}|",1,"Cistern Pressure Signal Under Range","RTN - Cistern Pressure Signal Normal",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_cysPress_faults_chan_out","Cistern Pressure IO Channel Fault","rosebud_feeders","mill","|{register:mill:water_g_cysPress_faults_chan_out}|",1,"Cistern Pressure IO Channel Fault","RTN - Cistern Pressure IO Channel OK",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_well4Flow_faults_over_out","Well 4 Flow Over-Range Fault","rosebud_feeders","mill","|{register:mill:water_g_well4Flow_faults_over_out}|",1,"Well 4 Flow Signal Over Range","RTN - Well 4 Flow Signal Normal",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_well4Flow_faults_under_out","Well 4 Flow Under-Range Fault","rosebud_feeders","mill","|{register:mill:water_g_well4Flow_faults_under_out}|",1,"Well 4 Flow Signal Under Range","RTN - Well 4 Flow Signal Normal",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_well4Flow_faults_chan_out","Well 4 Flow IO Channel Fault","rosebud_feeders","mill","|{register:mill:water_g_well4Flow_faults_chan_out}|",1,"Well 4 Flow IO Channel Fault","RTN - Well 4 Flow IO Channel OK",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_well4Lvl_faults_over_out","Well 4 Level Over-Range Fault","rosebud_feeders","mill","|{register:mill:water_g_well4Lvl_faults_over_out}|",1,"Well 4 Level Signal Over Range","RTN - Well 4 Level Signal Normal",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_well4Lvl_faults_under_out","Well 4 Level Under-Range Fault","rosebud_feeders","mill","|{register:mill:water_g_well4Lvl_faults_under_out}|",1,"Well 4 Level Signal Under Range","RTN - Well 4 Level Signal Normal",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_well4Lvl_faults_chan_out","Well 4 Level IO Channel Fault","rosebud_feeders","mill","|{register:mill:water_g_well4Lvl_faults_chan_out}|",1,"Well 4 Level IO Channel Fault","RTN - Well 4 Level IO Channel OK",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_cysLevel_limits_hihi_alm_out","Cistern Level High-High Alarm","rosebud_feeders","mill","|{register:mill:water_g_cysLevel_limits_hihi_alm_out}|",1,"Cistern Level Critically High","RTN - Cistern Level Back Below High-High",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_cysLevel_limits_hi_alm_out","Cistern Level High Alarm","rosebud_feeders","mill","|{register:mill:water_g_cysLevel_limits_hi_alm_out}|",1,"Cistern Level High","RTN - Cistern Level Back Below High",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_cysLevel_limits_lo_alm_out","Cistern Level Low Alarm","rosebud_feeders","mill","|{register:mill:water_g_cysLevel_limits_lo_alm_out}|",1,"Cistern Level Low","RTN - Cistern Level Back Above Low",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_cysLevel_limits_lolo_alm_out","Cistern Level Low-Low Alarm","rosebud_feeders","mill","|{register:mill:water_g_cysLevel_limits_lolo_alm_out}|",1,"Cistern Level Critically Low","RTN - Cistern Level Back Above Low-Low",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_cysPress_limits_hihi_alm_out","Cistern Pressure High-High Alarm","rosebud_feeders","mill","|{register:mill:water_g_cysPress_limits_hihi_alm_out}|",1,"Cistern Pressure Critically High","RTN - Cistern Pressure Back Below High-High",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_cysPress_limits_hi_alm_out","Cistern Pressure High Alarm","rosebud_feeders","mill","|{register:mill:water_g_cysPress_limits_hi_alm_out}|",1,"Cistern Pressure High","RTN - Cistern Pressure Back Below High",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_cysPress_limits_lo_alm_out","Cistern Pressure Low Alarm","rosebud_feeders","mill","|{register:mill:water_g_cysPress_limits_lo_alm_out}|",1,"Cistern Pressure Low","RTN - Cistern Pressure Back Above Low",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_cysPress_limits_lolo_alm_out","Cistern Pressure Low-Low Alarm","rosebud_feeders","mill","|{register:mill:water_g_cysPress_limits_lolo_alm_out}|",1,"Cistern Pressure Critically Low","RTN - Cistern Pressure Back Above Low-Low",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_well4Flow_limits_hihi_alm_out","Well 4 Flow High-High Alarm","rosebud_feeders","mill","|{register:mill:water_g_well4Flow_limits_hihi_alm_out}|",1,"Well 4 Flow Critically High","RTN - Well 4 Flow Back Below High-High",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_well4Flow_limits_hi_alm_out","Well 4 Flow High Alarm","rosebud_feeders","mill","|{register:mill:water_g_well4Flow_limits_hi_alm_out}|",1,"Well 4 Flow High","RTN - Well 4 Flow Back Below High",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_well4Flow_limits_lo_alm_out","Well 4 Flow Low Alarm","rosebud_feeders","mill","|{register:mill:water_g_well4Flow_limits_lo_alm_out}|",1,"Well 4 Flow Low","RTN - Well 4 Flow Back Above Low",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]
["water_g_well4Flow_limits_lolo_alm_out","Well 4 Flow Low-Low Alarm","rosebud_feeders","mill","|{register:mill:water_g_well4Flow_limits_lolo_alm_out}|",1,"Well 4 Flow Critically Low","RTN - Well 4 Flow Back Above Low-Low",2,{"$f":"FALSE()","v":false},0,0,{"$f":"TRUE()","v":true},"[\"194a9a6d-a4ee-45a3-a10b-90a2f76580b0\"]"]