{"payload":{"meta":{"Graph":{"@Type":"81297157","@Value":{"Guid":"(Guid)ce4ff206-b722-40a6-bd0e-2cfaa1b953f7","ParentGuid":"(Guid)74ccca2f-50e3-4d5a-9d7a-9fd420284f83","Name":"(string)atAlarm","Properties":{"@Type":"2c41fa04:IDictionary","@Value":[{"@Key":"(Guid)829a18f2-c514-4f6e-9634-1df173429203","@Value":{"@Type":"829a18f2","@Value":{"ParentObjects":{"@Type":"fa2ee218:IDictionary","@Value":[{"@Key":"(Guid)d9b2b2cc-ea99-4c3b-aa42-1e5c49e65b84","@Value":"(Guid)2f85e93d-ece0-4c49-90fd-157464c53ecc"}]}}}}]},"TypeGuid":"(Guid)6f9dac99-8de1-4efc-8465-68ac443b7d08","EmbeddedTypeGuids":{"@Type":"[Guid]","@Value":["(Guid)a9ed5b7e-75c5-4651-af16-d2c27e98cb94","(Guid)3b83b776-fb25-43b8-99f2-3c507c9143fc"]}}},"TypeInfos":{"2c41fa04":"{2c41fa04-1834-41c1-816e-303c7aa2c05b}","81297157":"{81297157-7ec9-45ce-845e-84cab2b88ade}","829a18f2":"{829a18f2-c514-4f6e-9634-1df173429203}","fa2ee218":"{fa2ee218-a39b-4b6d-b249-49dbddbd168a}","Guid":"System.Guid","string":"System.String"}},"object":{"Graph":{"@Type":"6f9dac99","@Value":{"SpecialFunc":{"@Type":"0db3d7bb:Enum","@Value":"None"},"Implementation":{"@Type":"3b83b776","@Value":{"TextDocument":{"@Type":"f3878285","@Value":{"TextBlobForSerialisation":"(string)//Alarm logic\n//2024-02-13 CWD Added debounce and enable\n//2024-04-29 CWD Fix en was set as in output, changed to an input\n//2024-08-13 CWD Add default output, this is specified in the program as either latched or unlatched\n//2024-11-15 ATM Update to new in_ out_ schema\n\n//Turn of everything if not enabled\nIF NOT in_enProc THEN\n\tin_raw := FALSE;\n\tlast := FALSE;\n\tdebounced := FALSE;\nEND_IF\n\n//Debounce function\ntimOn(IN := in_raw = TRUE AND last = FALSE, PT := in_delOn);\ntimOff(IN := in_raw = FALSE AND last = TRUE, PT := in_delOff);\nIF timOn.Q OR timOff.Q THEN\n\tlast := in_raw;\n\tdebounced := in_raw;\nEND_IF\n\n//unlatched follows in\nout_unlatched := debounced;\n\n//Latched is set on in = true, cleared on reset or not enabled\nIF in_reset THEN\n\tout_latched := FALSE;\nEND_IF\nIF debounced THEN\n\tout_latched := TRUE;\nEND_IF\n\n//Update the default output\nIF in_defaultType = atAlarmDefault.latched THEN\n\tout_default:= out_latched;\nELSE\n\tout_default:= out_unlatched;\nEND_IF","LineInfoPersistence":"(string)ce4ff206-b722-40a6-bd0e-2cfaa1b953f7_Impl_LineIds"}}}},"Interface":{"@Type":"a9ed5b7e","@Value":{"TextDocument":{"@Type":"f3878285","@Value":{"TextBlobForSerialisation":"(string){attribute 'no_assign'}\nFUNCTION_BLOCK atAlarm\nVAR_INPUT\n\tin_raw: BOOL;\n\tin_reset: BOOL;\n\t// Process controlled enable. eg only enable rpm lo when motor running\n\t{attribute 'symbol' := 'none'}\n\tin_enProc: BOOL := TRUE;\n\tin_defaultType: atAlarmDefault := atAlarmDefault.latched;\n\tin_almIDX: INT;\nEND_VAR\nVAR_INPUT PERSISTENT\n\tin_delOn: TIME := T#0S;\n\tin_delOff: TIME := T#1S;\nEND_VAR\nVAR_OUTPUT\n\tout_latched: BOOL; //Alarm will remain active until reset\n\tout_unlatched: BOOL; //Alarm will reset when source resets\n\tout_default: BOOL; //Latched or unlatched as specified in the program\nEND_VAR\nVAR\n\t{attribute 'symbol' := 'none'}\n\tdebounced: BOOL;\n\t{attribute 'symbol' := 'none'}\n\ttimON: TON;\n\t{attribute 'symbol' := 'none'}\n\ttimOff: TON;\n\t{attribute 'symbol' := 'none'}\n\tlast: BOOL;\nEND_VAR\n","LineInfoPersistence":"(string)ce4ff206-b722-40a6-bd0e-2cfaa1b953f7_Decl_LineIds"}}}},"UniqueIdGenerator":"(string)903","POULevel":{"@Type":"8e575c5b:Enum","@Value":"Standard"},"ChildObjectGuids":{"@Type":"ArrayList:IList","@Value":[]},"AddAttributeSubsequent":"(bool)False"}},"TypeInfos":{"0db3d7bb":"{0db3d7bb-cde0-4416-9a7b-ce49a0124323}","3b83b776":"{3b83b776-fb25-43b8-99f2-3c507c9143fc}","6f9dac99":"{6f9dac99-8de1-4efc-8465-68ac443b7d08}","8e575c5b":"{8e575c5b-1d37-49c6-941b-5c0ec7874787}","a9ed5b7e":"{a9ed5b7e-75c5-4651-af16-d2c27e98cb94}","ArrayList":"System.Collections.ArrayList","bool":"System.Boolean","f3878285":"{f3878285-8e4f-490b-bb1b-9acbb7eb04db}","string":"System.String"}}},"FormatVersion":"1.0"}